Readme1st
The A01 release of the C5765cdn cloning file.

This .zip file contains the files to be used for conversion of a standard Dell C5765cdn to a CACStar enabled machine.  
Files included are:
1.	C5765_Readme1st.txt - This document of usage
2.	CACStarAuthPlugin_A00.jar -
	Use of this file is described on Page 11 Step 9 of the Installation and Configuration Guide.
3.	CACStarService_Installer_A00.exe - 
	Use of this file is described on Page 11 Step 10 of the Installation and Configuration Guide.
4.	C5765-Cloning_A01.dat - 
	Use of this file is described on Page 12 Step 12 of the Installation and Configuration Guide.

******
Refer to the Dell C5765dn CACStar Smart Card Reader Installation and Configuration Guide for use of these files.   
The section called "Converting a Dell C5765dn to a CACStar Enabled Machine" provide specific steps for use of these files.
	Use of this file is described on Page 12 Step 12 of the Installation and Configuration Guide.

***** IMPORTANT INFORMATION *****

Additional information for the C5765-Cloning_A01.dat
 The A01 clone file is in compliance with DoD Ipv4 Security Technical Implementation Guideline (STIG). Release: 10 Benchmark Date:  28 July 17

"*" NOTES ADMINSTRATOR ATTENTION

PER STIG ID MFD01.001 - We have have set the protocols to reflect proper service of the 5765.  In question:  USB is enabled for Power purposes, SOAP is an internal protcol for applications to work with Web Services. 
PER STIG ID MFD02.004 - Always Recommended to have current firmware on the devices.  Please refer to: http://support.dell.com for the latest updates to firmware
*Per STIG ID MFD02.001 - Administrator will have to configure SNMP values.  To update printer firmware you will need to enable SNMPv1 and 2
PER STIG ID MDF02.002 -5765 will maintain its configuration state
*PER STIG ID MFD02.003 - HTTPS has been set per the installation instructions.  Administrator will have to enable SNMPv3 and shut down SNMPv1/2 
PER STIG ID MFD02.005 - Per VLAN operations or can be configured
PER STIG ID MFD03.001 - Set in the configuration STIG MFD01.001
PER STIG ID MFD04.001 - Per Administrator
PER STIG ID MFD05.001 - Per Administrator 
PER STIG ID MFD06.001 - Per Administrator 
PER STIG ID MFD06.001 - Per Administrator 
PER STIG ID MFD06.006 - Per Administrator 
PER STIG ID MFD07.001 - Per Administrator
PER STIG ID MFD07.002 - Per Administrator, FIPS 140-2 is activated  
PER STIG ID MFD07.003 - Per Administrator
PER STIG ID MFD07.004 - Per Administrator, Audit logs can be enabled for fax.  However the clone file did not have fax option installed
*PER STIG ID MFD07.005 - Per Administrator the the SMTP Server will be configured via CACStar.  Printer will retain a SMTP configuration of 172.19.10.1:25
PER STIG ID MFD08.001 - Per Administrator
PER STIG ID MFD08.002 - Per Administrator

*MAC Address
To obtain the MAC address of the CACStar unit, print out the Print Summary page found on CACStar configuration link found on the upper right hand side and then select Print Summary.
Additionally, CACStar unit produced with Firmware version A24 or greater, will have a gray sticker noting the Firmware version (ie. A28) and the MAC address. 





