; OEMSETUP.INF
;
; Kyocera Mita PCL Printer Driver
; Windows 2K/XP/2003
;
;  Copyright 2000-2002 KYOCERA CORPORATION
;  Copyright 2003-2004 Revised KYOCERA MITA CORPORATION
;  All Rights Reserved.

[Version]
Signature="$Windows NT$"
Provider=%KMC%
ClassGUID={4D36E979-E325-11CE-BFC1-08002BE10318}
Class=Printer
CatalogFile=KYOMITA.CAT
;
; Required by W2K Client/Server!!!
; Date must be in mm/dd/yyyy format
;
DriverVer  = 09/17/2004,3.8

[ClassInstall32.NT]
AddReg=printer_class_addreg

[printer_class_addreg]
HKR,,,,%PrinterClassName%
HKR,,Icon,,"-4"
HKR,,Installer32,,"ntprint.dll,ClassInstall32"
HKR,,NoDisplayClass,,1
HKR,,EnumPropPages32,,"printui.dll,PrinterPropPageProvider"


;
; OEM URLS
;
; This sections gives the URL for manufacturers found in the Manufacturers section
;
;[OEM URLS]
;%Kyocera_Mita% = "http://www.kyoceramita.de"


;
; Manufacturer section.
;
; This section lists all of the manufacturers
; that we will display in the Dialog box
;
[Manufacturer]
"Kyocera Mita"
; "Kyocera Mita KM"

;
; Model sections.


[Kyocera Mita]
"Kyocera Mita KM-1650" = KMKM1650.GPD,LPTENUM\KyoceraKM-16503A87,USBPRINT\KyoceraKM-16503A87,Kyocera_Mita_KM-1650

;
; Installer Sections
;
; These sections control file installation, and reference all files that
; need to be copied. The section name will be assumed to be the driver
; file, unless there is an explicit DriverFile section listed.

; Kyocera Mita KM
;

[KMKM1650.GPD]
CopyFiles=KMDLL_CopyFiles,@KMKM1650.GPD
DataFile=KMKM1650.GPD
DataSection=UNIDRV_BIDI_DATA
Include=NTPRINT.INF
Needs=TTFSUB.OEM,UNIDRV_BIDI.OEM

[KMDLL_CopyFiles]
KMRES2.DLL

;
; Copy Sections
;
; Lists of files that are actually copied. These sections are referenced
; from the installer sections, above. Only create a section if it contains
; two or more files (if we only copy a single file, identify it in the
; installer section, using the @filename notation) or if it's a color
; profile (since the DestinationDirs can only handle sections, and not
; individual files).

;
; Data Sections
;

;[OEM_BIDI_DATA]
;DriverFile=UNIDRV.DLL
;ConfigFile=UNIDRVUI.DLL
;HelpFile=UNIDRV.HLP
;LanguageMonitor=%OEM_MONITOR%

;[OEM_BIDIMON]
;OEMMON.DLL,,,0x00000020         ; Copy only if new binary

;
; Call SetupSetDirectoryId with 66000 to set the target directory at runtime
; (depending on which environment drivers are getting installed)
;

[DestinationDirs]
DefaultDestDir=66000
;OEM_COLOR1=66003
;OEM_COLOR2=66003


[SourceDisksNames.x86]
1   = %Disk1%,,,""

;[SourceDisksNames.Alpha]
;1   = %Disk1%,,,""


[SourceDisksFiles]
KMKM1650.GPD = 1
KMRES2.DLL   = 1


;
; Localizable Strings
;

[Strings]
KMC              = "Kyocera Mita"
PrinterClassName = "Printers"
Disk1            = "Kyocera Mita Digital Library CD-ROM"
