Samsung CLX-7450 Series/SCX-7500 Series/SCX-7300 Series

	Copyright(C) 2003-2005 TOSHIBA TEC CORPORATION All right reserved.
			January 15, 2005

This product has the following restrictions and issues.  Please be sure to read this before using.

--------------------------------------------------------------------------------
Installation
--------------------------------------------------------------------------------

Issues
======

1.CLX-7450 Series

1-1. In case that the SCX-7500 series or SCX-7300 series software has already been installed in your PC, please install the CLX-7450 series printer driver only.  You can continue to use Document Monitor and TWAIN/Filedownloader already installed in your PC with the SCX-7500 series or SCX-7300 series installer.
Or uninstall Document Monitor and TWAIN/FileDownloader of the SCX-7500 series or the SCX-7300 series before installing the CLX-7450 series software.

1-2. When you would like to install the SCX-7500 series or SCX-7300 series software in your PC in addition to the CLX-7450 series software which has already been installed, please install the SCX-7500 series or SCX-7300 series printer driver only.  You can continue to use Document Monitor and TWAIN/Filedownloader already installed in your PC with the CLX-7450 series installer.
Or uninstall Document Monitor and TWAIN/FileDownloader of the CLX-7450 series before installing the SCX-7500 series or the SCX-7300 series software.

1-3. New drivers and applications, which are installed from this CD-ROM, may not function properly if those of old Samsung/TOSHIBA products are already installed on a PC and are removed after the installation of new ones.  
In such a case, uninstall the new drivers and applications, then install them again using the CD-ROM.

1-4. When you install the printer driver and enter the NDS queue name for the Novell environment, enter as follows:
\\<NetWare server name>\<queue name>
Example: tree=org, context=dept1, queue name=mfp_queue
\\org\mfp_queue

1-5. If you need to set NetWare port as a printing port, input the port name manually.

1-6. Please update the CLX-7450 series client software after uninstalling the CLX-7450 series client software and the printer driver currently installed in your PC.

1-7. After you install the current version of the CLX-7450 series CD, do not perform additional installation or modification using any previous versions of the CLX-7450 series CD.

1-8. In Document Monitor Local Discovery while Client2 CD is being installed, the selection of devices is disabled by Discovery Settings. Select a desired model name from all the MFP model names detected.


2.SCX-7500 Series

2-1. In case that the CLX-7450 series or SCX-7300 series software has already been installed in your PC, please install the SCX-7500 series printer driver only.  You can continue to use Document Monitor and TWAIN/Filedownloader already installed in your PC with the CLX-7450 series or SCX-7300 series installer.
Or uninstall Document Monitor and TWAIN/FileDownloader of the CLX-7450 series or the SCX-7300 series before installing the SCX-7500 series software.

2-2. When you would like to install the CLX-7450 series or SCX-7300 series software in your PC in addition to the SCX-7500 series software which has already been installed, please install the CLX-7450 series or SCX-7300 series printer driver only.  You can continue to use Document Monitor and TWAIN/Filedownloader already installed in your PC with the SCX-7500 series installer.
Or uninstall Document Monitor and TWAIN/FileDownloader of the SCX-7500 series before installing the CLX-7450 series or the SCX-7300 series software.

2-3. New drivers and applications, which are installed from this CD-ROM, may not function properly if those of old Samsung/TOSHIBA products are already installed on a PC and are removed after the installation of new ones.  
In such a case, uninstall the new drivers and applications, then install them again using the CD-ROM.

2-4. When you install Client Softwares and enter the NDS queue name for Novell environmnet, enter as the following:
\\<NetWare server name>\<queue name>
Example: tree=org, context=dept1, queue name=mfp_queue
\\org\mfp_queue

2-5. If you need to set NetWare port as a printing port, input the port name manually.

2-6. Please update the SCX-7500 series client software after uninstalling the SCX-7500 series client software and the printer driver currently installed in your PC.

2-7. After you install the current version of the SCX-7500 Series CD, do not perform additional installation or modification using any previous versions of the SCX-7500 Series CD.

2-8. In Document Monitor Local Discovery while Client2 CD is being installed, the selection of devices is disabled by Discovery Settings. Select a desired model name from all the MFP model names detected.


3.SCX-7300 Series

3-1. In case that the CLX-7450 series or SCX-7500 series software has already been installed in your PC, please install the SCX-7300 series printer driver only.  You can continue to use Document Monitor and TWAIN/Filedownloader already installed in your PC with the CLX-7450 series or SCX-7500 series installer.
Or uninstall Document Monitor and TWAIN/FileDownloader of the CLX-7450 series or the SCX-7500 series before installing the SCX-7300 series software.

3-2. When you would like to install the CLX-7450 series or SCX-7500 series software in your PC in addition to the SCX-7300 series software which has already been installed, please install the CLX-7450 series or SCX-7500 series printer driver only.  You can continue to use Document Monitor and TWAIN/Filedownloader already installed in your PC with the SCX-7300 series installer.
Or uninstall Document Monitor and TWAIN/FileDownloader of the SCX-7300 series before installing the CLX-7450 series or the SCX-7500 series software.

3-3. New drivers and applications, which are installed from this CD-ROM, may not function properly if those of old Samsung/TOSHIBA products are already installed on a PC and are removed after the installation of new ones.
In such a case, uninstall the new drivers and applications, then install them again using the CD-ROM.

3-4. When you install Client Softwares and enter the NDS queue name for Novell environmnet, enter as the following:
\\<NetWare server name>\<queue name>
Example: tree=org, context=dept1, queue name=mfp_queue
\\org\mfp_queue

3-5. If you need to set NetWare port as a printing port, input the port name manually.

3-6. Please update the SCX-7300 series client software after uninstalling the SCX-7300 series client software and the printer driver currently installed in your PC.

3-7. After installing the current version of the SCX-7300 series CD, do not perform additional installation or modification using any previous versions of the SCX-7300 series CD.

3-8. In Document Monitor Local Discovery while Client2 CD is being installed, the selection of devices is disabled by Discovery Settings. Select a desired model name from all the MFP model names detected.


--------------------------------------------------------------------------------
SyncThru Web Service
--------------------------------------------------------------------------------

Issues
======

1. Netscape Navigator
- When Password Manager is used while using Netscape Navigator, any entries may seem not to be reflected.  Do not use Password Manager.

2. IP Address Setting
- Input for IP Address is 3 digits when MFP cannot be found by IP Address designation.
E.g.  192.254.10.5 -> 192.254.010.005

3. When the [Cancel] button is pressed on the SMTP Authentication setting screen, the screen until the [Cancel] button is pressed becomes valid.


--------------------------------------------------------------------------------
Printer Driver

CLX-7450 Series	for Windows(PCL5c/PCL6/PSL3)		Version 1.21.8.0
			for Macintosh PPD(OS8.6/9)		Version 1.00
			for Macintosh PPD(OS-X10.2.*/10.3.*)	Version 1.00
			for UNIX/LINUX Filter			Version 1.01

SCX-7500 Series	for Windows(PCL6/PSL3)			Version 1.21.8.0
			for Macintosh PPD(OS8.6/9)		Version 1.00
			for Macintosh PPD(OS-X10.2.*/10.3.*)	Version 1.00
			for UNIX/LINUX Filter			Version 1.01

SCX-7300 Series	for Windows(PCL6/PSL3)			Version 1.21.8.0
			for Macintosh PPD(OS8.6/9)		Version 1.00
			for Macintosh PPD(OS-X10.2.*/10.3.*)	Version 1.00
			for UNIX/LINUX Filter			Version 1.01
--------------------------------------------------------------------------------

Issues
======

1. Windows
- When Portrait and Landscape images exist on the same sheet in "Multiple Pages per Sheet" printing, printing will be performed by reducing, not by rotating the images.

- When the duplex printing and the Back Cover are set as a combination on Windows 98 and Windows Me, the image on the Back Cover may not be rotated or printed on correct sized paper.

(CLX-7450 Series)
- When an original paper, which contains Portrait and Landscape images, is printed in the 2-Sided Printing mode using the PostScript driver, an image may be printed on the next page when orientation of the image changes.  In such a case, perform printing using the PCL5c driver.

(SCX-7500 Series/SCX-7300 Series)
- When an original paper, which contains Portrait and Landscape images, is printed in the 2-Sided Printing mode using the PostScript driver, an image may be printed on the next page when orientation of the image changes.  In such a case, perform printing using the PCL6 driver.

- Help message does not appear even when the "?" button on the upper right of the screen is clicked.
- When using a Standard TCP/IP port under Windows 2000/XP, do not change the default port name.  If the port name should be changed, change the name, open the Property of the printer driver and click on the Configuration tab, then Update Now button to find e-STUDIO currently being used.

- When printing is performed in a NetWare environment, SNMP communication cannot be performed immediately after the printer driver is installed.  Open the Property of the printer driver and click on the Configuration tab, then Update Now button to find e-STUDIO currently being used.

- SNMP communication cannot be performed immediately after the printer driver is installed on Windows98/Me from the Windows NT/2000/2003 server by Point & Print.  Open the Property of the printer driver and click on the Configuration tab, then Update Now button to find e-STUDIO currently being used.

- Do not use NetCrawl function in WindowsMe.

- When the PSL3 Printer Driver is used with Adobe TypeManager Font, an error will result.  So do not use Adobe TypeManager Font.  Use the PCL Printer Driver when you need to use Adobe TypeManager Font.

- When a modem is used, the dial-up connection dialog may appear during printing from Windows 98/Me.

- When LPR is used for printing, disable Byte Counting.

(SCX-7300 Series)
- When using NetWare 5.x Server in a NDPS environment, the PSL3 printer driver may not be automatically downloaded on Windows 98/Me.  In such a case, install the PSL3 printer driver directly from the CD-ROM.

(SCX-7300 Series)
- When printing a Watermark, the result may not be as you had expected depending on the settings.  In such a case, print the Watermark again after changing the size and position of the Watermark.  It is effective to position the Watermark in the printable area.

(SCX-7300 Series)
- When the PCL6 driver is used and "Always Use TrueType Fonts" is selected, the character pitch may be increased or characters may be deformed depending on the font being used for the original.  To solve this problem, change the setting to "Use Font Substitution Table".


- Printing from an application

(1) Overview
Although some printing options can be set from your application, do not use your application to set printing. Use your printer driver to set printer options.
When printing is performed after setting such options in your application, you may end up with an unexpected result or it may take a long time to process.
Do not set "Collate" in your application.
When setting a paper tray in your application, two "AutoSelect tray"s may be displayed. In this case, select the lower "AutoSelect tray."

(CLX-7450 Series)
When the print setting is changed from monochrome printer driver to CLX-7450 Series PCL5c/PSL3 Printer Driver, Mono setting may remain in Setup tab on some applications.  To perform color printing, select Automatic before printing.

(2)Microsoft Office
When the error sheet describing ERROR: limitcheck or ERROR: VMerror is printed during printing from Microsoft Office 2003 using the PS Driver, turn the e-STUDIO off then on.
If the same error persists during re-printing, uncheck [Use PostScrip Passthrough], or use the PCL6 Driver.

(2-1) Microsoft PowerPoint
Set the "Number of copies" by using the PowerPoint. Do not use your printer driver to set it. 
The number of copies set in PowerPoint overwrites the default setting of the Windows 98/Me and Windows NT4.0 printer driver.

(CLX-7450 Series)
To print PowerPoint documents in colors, select Color in PowerPoint's Print dialog and select Automatic in printer driver's Setup tab.

(2-2) Microsoft Excel
Excel handles each worksheet as one print job.  The settings on the printer driver screen apply to the first worksheet only.

When you enter more than one in [Copies] on the Print dialog for Excel, do not check [Collate].

(CLX-7450 Series/SCX-7500 Series)
(3) Adobe Acrobat 6.0
When PSL3 is used for printing, a printed image may be enlarged or reduced.  In such cases, using PCL5c/PCL6 or using PSL3 with the following setting can print the image at a proper size.
Open the Print dialog box to perform the setting for PSL3.
- Select [Fit to Paper] form from the [Page Scaling] menu.
- Check [Choose Paper Source by PDF page size].
(Note that the driver's paper setting is not valid as the PDF file's paper size is used.)


- Point and print from the Windows Server

(1) Printing setup that is set in "Printing Defaults" of the server cannot be reflected to the client side depending on the combination of the server OS and the client OS.


2. Macintosh Printing

OS8.6/9:

- When printing from Adobe Photo Shop 5.5, there is no file to store your desired job. Please disable 8-bit printing in Print Setup and change encoding to ASCII (not BINARY).

- The "Collate" setting will not be saved when saving the printer default setup.

- All stapling options are displayed even though some are unavailable.  For example, you can select "Middle Left" stapling even when you are using A3. As you cannot staple on the long edge of the A3, your job will not be stapled.  However, the job will get printed.

- When you designate the paper size in the page setting, the paper size such as A4 or Letter may not be displayed and "Others" may be displayed.  In this case, the setting cannot be returned to "Others" if the size is changed to another one by clicking "OK". Or you can do this by designating another "Format for". 

-After a printer is added by "Desktop Printer Utility" and printing is performed without changing the installable options or printing setup, printing cannot be done in a designated paper size in the "Page Setup".

(CLX-7450 Series/SCX-7500 Series)
- When printing the Adobe PageMaker file, Department Code is not acceptable.

(SCX-7300 Series)
- For using the Cover function on Macintosh OS-9, use AppleTalk connection.

OS-X:

- All stapling options are displayed even though some are unavailable.  For example, you can select "Portrait A4 Left Hand Side" stapling even when you are using A3. As you cannot staple on the long edge of the A3, your job will not be stapled. However, the job will get printed.

- When the print is executed on Mac OS-X 10.2, the function set may be reduced from the printer functions or the set items may be deleted. Since this is an OS problem, you would need to re-start the OS to correct it.

(SCX-7300 Series)
- When using Macintosh and perform printing from an Adobe Acrobat PPD file on a paper of which size is other than Letter or A4 and the paper source to be used is specified, printing may be performed on Letter or A4 size paper fed from the Bypass Feeder.  When printing on a paper other than Letter or A4, set the paper source to Auto.

- Setting control of Destination and Stapling/Hole Punch do not work correctly due to a problem in the printing function of Mac OS-X 10.2.*.
Therefore, Inner Tray and Stapling/Hole Punch can be set up at the same time.
Paper will be output to Inner Tray and Stapling/Hole Punch cannot be performed. 
When handling Stapling/Hole Punch, please set Tray 1 or Tray 2 as your Destination.

- When you designate the paper size in the page setting, the paper size such as A4 or Letter may not be displayed and "Others" may be displayed. In this case, the setting cannot be returned to "Others" if the size is changed to another one by clicking "OK". Or you can do this by designating another "Format for".

- When saving printer Presets on Mac OS-X 10.2, the setup is not saved unless preview or printing is executed.
Even if two or more Presets were saved, the last setup saved with Printer Features is only available.

- This PPD does not support Rendezvous printing.
When you use Print Center to set up the printer via Rendezvous, the setup does not terminate although this PPD is selected.

- When printing from Macintosh, "OSX USER" is displayed as a user name for the print job on the control panel.

3. Unix/Linux Filter

- All stapling options are displayed even though some are unavailable.  For example, you can select "Portrait A4 Left Hand Side" stapling even when you are using A3.
As you cannot staple on the long edge of A3, your job will not be stapled.
However the job will get printed.

4. Banner Page
- Banner page will be output onto a tray that had been designated in RAW Jobs - Default Output Tray in TopAccess.


--------------------------------------------------------------------------------
Print
--------------------------------------------------------------------------------

Issues
======

1. Some documents may cause print-assigned memory to become insufficient to print.

2. When an error sheet is printed, subsequent print jobs may not be printed properly.  In this case, turn the MFP off then on.

(CLX-7450 Series)
3. When printing is performed with the PS3/PCL5c in color mode, grey areas are printed with the black toner.  This is because the default setting of printer driver's "Pure Grey" under "Image Quality" is set to ON.  This may result in unexpected print output (for example, smooth gradation may change to striped pattern, depending on print data.  To solve this problem, set "Pure Grey" to OFF.


--------------------------------------------------------------------------------
Document Monitor

CLX-7450 Series				Version 1.21.49.3
SCX-7500 Series				Version 1.21.49.3
SCX-7300 Series				Version 1.21.49.3
--------------------------------------------------------------------------------

Issues
======

1. Not discover any device(s)

[Problem Description]
Document Monitor Local Discovery and Network Discovery may not search some device(s)
(E.g. Devices(s) with a different segments)

[Corrective Action]
Click the "Manual Selection" button on the Discovery dialog, and enter Printer Name and the IP/IPX Address.

2. When a message "No Default Printer" displays.

[Problem Description]
When the printer driver is not installed and Document Monitor cannot obtain the correct port value, the message, "No Default Printer" displays.

[Corrective Action]
Check your printer driver and printer that are used normally. Or restart Document Monitor.

3. Event Notification

[Problem Description]
When Novell client and IPX/SPX protocol are installed on your PC and NDS/NDPS is used, an event notification may not be displayed.

[Corrective Action]
Check a list which shows the print status and device status in the Document Monitor window.

4. Document Pages

[Problem Description]
When printing is performed by the CLX-7450 series, the SCX-7500 series or the SCX-7300 series, the number of pages that is displayed in the job status will be "total pages / total pages". 


--------------------------------------------------------------------------------
TWAIN Driver/File Downloader

CLX-7450 Series				Version 1.21.42.0
SCX-7500 Series				Version 1.21.42.0
SCX-7300 Series				Version 1.21.42.0
--------------------------------------------------------------------------------


To use the TWAIN driver with the application, individual configurations may be necessary. Configure by referring to the following configuration or the application manual.

1. The imaging application for Windows NT does not support capturing through TWAIN.

2. The imaging application for other Windows OS does not support multiple-paged originals with mixed colors or sizes.

3. TextBridge/OmniPage
Configure the following in the "Scanner setup wizard":
   1. Select "Show TWAIN Interface" in the "Advanced" configuration.
   2. Store one-paged original in the e-Filing box before testing the scanner.

4. Applications such as Acrobat 6.0 do not support capturing through TWAIN; depending on colors, paper sizes, or several originals with mixed resolutions.  To capture an image using such applications, capture each page individually or use the FileDownloader to save the same document first.  Then open it from applications such as TIFF/PDF.


Issues
======

1. Accessing performance may decline when the e-Filing Box has many documents. We recommend you to decrease the number of documents by separating folders or boxes.

2. Performance of deleting pages from a document may decline when that document contains a large number of pages.


3. Retrieving a color image will require huge memory. Performance may decline or imaging may end in failure when imaging is performed with low memory.  Necessary space of memory for color image is approx. 100 MB for A4/LT or 200 MB for A3/LD in 600dpi.  The recommended memory size for the client PC is 256 MB or more to retrieve A4/LT pages, or 512 MB or more to retrieve A3/LD pages.


Troubleshooting
===============

1. Cannot Find the MFP (TWAIN/FileDownloader)

[Problem Description]
Cannot find the MFP even when the Local Discovery or Network Discovery feature is used.

[Corrective Action]
Confirm the following:
- The MFP and your PC are correctly connected to the TCP/IP network.
- The default gateway setting is correctly set up if the MFP is connected to a different subnet.

2. Cannot Connect to the MFP Found by the Local Discovery (TWAIN/FileDownloader)
    	
[Problem Description]
The Local Discovery finds the MFP, but you cannot connect to it.

[Corrective Action]
1. Make sure Microsoft Internet Explorer 5.5 or later is installed.
2. Make sure the Proxy settings on the Microsoft Internet Explorer have been made correctly so that your PC can connect to the MFP.
3. Make sure Microsoft Internet Explorer is not in the off-line mode. If it is in off-line mode, change it to the on-line mode.
    
[NOTE]
- Connection to the MFP may fail when too many PCs connect to the MFP at the same time. 
- Please try to connect to the MFP again later.

3. Cannot Acquire Document (TWAIN)
    
[Problem Description]
Cannot acquire a document using the TWAIN Driver.

[Corrective Action]
The TWAIN Driver has been carefully tested with several TWAIN-compliant applications. However, some applications may require settings to connect to the TWAIN driver, or some applications that have not been tested cannot connect to the MFP.  See the Readme file for the required settings in applications that have been tested.  Also, an application that has not been tested may operate by enabling the Native UI of the TWAIN Driver or changing the Data Transfer Mode.  For more details about TWAIN settings on your application, see the user manual for your application.

4. Image Corrupts When Acquiring Color Mixed Document (TWAIN)

[Problem Description]
An image will become corrupted when capturing the document that contains both color pages and black and white pages, using the TWAIN driver.
    
[Corrective Action]
Capturing a color and black/white mixed document is not supported by some applications.  In that case, capture the color pages and black and white pages separately or store the document as a file using the FileDownloader.

5. Saved as Single Page Files Even Though You Select Multi Page
   TIFF Format (File Downloader)

[Problem Description]
When storing a document in a Multi-page TIFF format using the File Downloader, the document is stored in single-page.

[Corrective Action]
The FileDownloader cannot save the color and black/white mixed document as a multi page TIFF file. In that case, the FileDownloader saves the document as single page files.  In this case, a color document is stored in JPEG format.  If you want to save the document as one file, save it as a PDF file.

6. Cannot Open TIFF File Saved Using FileDownloader (FileDownloader)

[Problem Description]
Cannot open the TIFF file that has been saved using the FileDownloader.

[Corrective Action]
When you select a TIFF format to save the color/grayscale document using the FileDownloader, the document will be saved as TIFF file with JPEG compression.  You cannot open the file using an application that does not support the TIFF file with JPEG compression.  In that case, save the document as a JPEG file or use the TWAIN driver to capture the document.

7. Cannot Change Resolution by Shrink To Half (TWAIN/FileDownloader)

[Problem Description]
Even though you enable the Shrink to Half function, the	resolution of an image that was acquired is not changed.

[Corrective Action]
The Shrink to Half function is available only for 600x600dpi documents that are stored in e-Filing by copy and print operations. This function cannot reduce the resolution of the image that is saved by scan and fax operation. You can change the resolution of the image in the filing box, by faxing or scanning it again at your desired resolution and storing it in the filing box, or by changing the resolution in the application.

8. Cannot Acquire Multi-Paged Document (TWAIN)

[Problem Description]
Cannot acquire a multi-paged document from an application.

[Corrective Action]
Some applications do not support multi page scan from TWAIN interface or need to be configured to acquire multi-paged documents.  See the user documentation for the application that you use.

9. Refresh Button Keeps Returning Error (TWAIN/FileDownloader)

[Problem Description]
Refresh action does not reconnect to MFP and keeps returning error.

[Corrective Action]
This behavior is caused by mismatch between the MFP status and the driver internal status.  To solve this problem, please select the MFP again by selecting "Box Select"->"Select e-STUDIO" or restart the driver.

10. Cannot Connect to the Device (TWAIN/FileDownloader)

[Problem Description]
When you start TWAIN driver of FileDownloader installed in the WindowsMe, an error message, "Connection to MFP has aborted", displays and you cannot connect to the Device.

[Corrective Action]
When you are using the WindowsMe and if the TCP/IP network default gateway is not set, you may fail connecting in the network.
Set the default gateway by using the network-setting tool in the control panel.


--------------------------------------------------------------------------------
Network Fax Driver

CLX-7450 Series				Version 1.21.8.0
SCX-7500 Series				Version 1.21.8.0
SCX-7300 Series				Version 1.21.8.0
--------------------------------------------------------------------------------

Issues
======

1. When you use the port created using the peer-to-peer utility, telephone numbers cannot be specified for destinations.  Use a local or other ports.

(SCX-7300 Series)
2. Do not use the N/W Fax front page function in the Windows98/Me environment.


--------------------------------------------------------------------------------
AddressBook Viewer

CLX-7450 Series				Version 1.21.50.4
SCX-7500 Series				Version 1.21.50.4
SCX-7300 Series				Version 1.21.50.4
--------------------------------------------------------------------------------

Issues
======

1. LDAP Server
LDAP supports the following schema.
	Surname:	sn
	Name:		cn
	Company name:	o, company, companyname
	Department:	ou, department
	E-mail address:	mail
	Fax number:	facsimileTelephoneNumber

2. Restrictions when Network-Fax is install as a print server
When Network-Fax is used as a print server, whether or not the Fax number and e-mail address can be used is unclear since MFP's option configuration cannot be confirmed.
When the CLX-7450 series, the SCX-7500 series or the SCX-7300 series is locally connected, the status of the options (FAX board, Printer kit or Scanner upgrade kit) may not be confirmed, since AddressBook Viewer acquires the machine status through the SNMP protocol.  Select the destination after confirming the equipment configuration.

3. When MFP's address book is changed after downloading Public AddressBook, destinations may differ between Public AddressBook and MFP's address book.  In this case, Network-Fax is not sent to destinations that do not exist in MFP's address book, due to the security policy.
In this case, check the message log through TopAccess.  The following error message is shown.
"Security error on eSTUDIO Address Book" (Error Code 5C11)
When this error occurs or the MFP's address book is changed, download Public AddressBook again.

4. When AddressBook Viewer is started on Network-Fax, while the client PC is Windows 98/Me, the error message indicating the server is being used may appear.  In this case, start AddressBook from the menu bar in order to perform equipment setting.

5. MAPI Setting
For MAPI connected server setting, refer to the respective manual for each server.
MAPI address book is supported by Outlook 2002 or later.

(SCX-7300 Series)
6. Caution for Converting Address Book
A CSV file before and after converting the address book cannot be edited.

7. You would need to import the CSV file by AddressBook Viewer, which you have exported in SyncThru Web Service, to acquire over 1,000 addresses for Public AddressBook.


--------------------------------------------------------------------------------
e-Filing
--------------------------------------------------------------------------------

Issues
======

1. The Document archive function is not supported by Netscape 4.76 and Netscape 6.2.2. Use Netscape 7.1 or higher.

2. Edited documents cannot be stored when using Netscape 6.2.2. Use Netscape 7.1 or higher.


--------------------------------------------------------------------------------
Email Notification
--------------------------------------------------------------------------------

Issues
======

1. Even if Door/Drawer Open is checked in General Notification Events for Email Notification, Email Notification is not made by Drawer Open.


--------------------------------------------------------------------------------
Message Log Function
--------------------------------------------------------------------------------

Issues
======

1. Even if Drawer Open is performed, Message Log is not displayed.


--------------------------------------------------------------------------------
Network
--------------------------------------------------------------------------------

Issues
======

1. When the following occurs after changing network setting, turn off the MFP and then on.

(1) When the "NETWORK INITIALIZING" display remains on the panel.
(2) Network settings are not properly reflected.
(3) Network settings cannot be changed.

2. When mail server POP3 login has failed with "Auto" selected, try it again after setting Type POP3 Login to "POP3" or "APOP".  After changing the setting, turn the MFP power OFF and On again.


--------------------------------------------------------------------------------
SMB Print and SMB Print in Point & Print
--------------------------------------------------------------------------------

Issues
======

1. SMB Print and SMB Print in Point & Print are intended for use in a small-scale network.  When your environment allows Windows NT 4.0, Windows 2000, or Windows XP to be used as a print server, it is recommended you print via the Windows print server.

2. When several users install the driver through the Point & Print function at the same time, an error message or any screen prompting you to install the driver from the CD may be displayed during downloading.  Retry downloading after making sure other users have completed downloading.
While installing the printer driver to your PC, ask other PC users not to send print jobs, if possible.  Close a print queue immediately after installation is completed.

3. After installing the printer driver by the Point & Print function, make sure that printing can be performed successfully by printing a test page.  If printing has failed, uninstall the printer driver, and install it again after restarting your PC.  For uninstallation, refer to the Printing Guide, "Uninstalling the Client1 Software" - "When Installed Using Add Printer Wizard".

4. Printer queue may be brought offline on the client PC during printing from Windows 98 or Windows Me.  Bring it online again.

5. When printing cannot be performed with Point & Print, it is recommended to perform SMB print if Windows98 or WindowsMe is used and LPR print for other OS.

6. When updating the printer driver through the Point & Print function, uninstall the current printer driver installed using the Point & Print function, restart the PC, then install a new printer driver.  For uninstallation, refer to the Printing Guide, "Uninstalling the Client1 Software" - "When Installed Using Add Printer Wizard".


--------------------------------------------------------------------------------
Trademarks
--------------------------------------------------------------------------------

- The official name of Windows 98 is Microsoft Windows 98 Operating System.
- The official name of Windows Me is Microsoft Windows Me Operating System.
- The official name of Windows 2000 is Microsoft Windows 2000 Operating System.
- The official name of Windows XP is Microsoft Windows XP Operating System.
- Microsoft, Windows, Windows NT, and the brand names and product names of other Microsoft products are trademarks of Microsoft Corporation in the US and other countries.
- Apple, AppleTalk, Macintosh, Mac, TrueType, and LaserWriter are trademarks of Apple Computer Inc. in the US and other countries.
- Postscript, and the brand names and product names of other Adobe Systems products are trademarks of Adobe Systems Incorporated in the US and other countries.
- Netscape is a trademark of Netscape Communications Corporation.
- IBM, AT and AIX are trademarks of International Business Machines Corporation.
- Novell, NetWare, and NDS are trademarks of Novell, Inc.
- Other company names and product names in this manual are the trademarks of their respective companies.
